[Contents] [Prev] [Next] [Index] [Report an Error]

# show ipv6 route

#### Syntax

show ipv6 route [ vrf vrfName ] [ ipv6Address [ detail ] | ipv6Prefix [ detail ] ] [ all ]
[ protocol ] [ filter ]

To display summary information:

show ipv6 route summary [ vrf vrfName ] [ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
vrf keyword and vrfName variable added in JUNOSe Release 7.2.0.

#### Description

Displays current state of the IPv6 routing table.

#### Options

- vrfName—Name of the VRF
- ipv6Address—IPv6 address
- ipv6Prefix—Prefix of prefix list entry; in the format IPv6baseaddress / length; for example, 1::1/32
- detail—Displays detailed information about the specific route
- all—Displays routes from all sources to a prefix
- protocol—One of the following protocols for which you want to display the best routes in the routing table; no routes are displayed if routes for the specified protocol are not present in the routing table
  - access—Displays the best access-server routes (BGP) in the routing table
  - access-internal—Displays the best access-internal routes in the routing table
  - bgp—Displays the best BGP routes in the routing table
  - bgp-tunnel—Displays the best BGP tunnel routes in the routing table
  - dvmrp—Displays the best DVMRP routes in the routing table
  - isis—Displays the best IS-IS routes in the routing table
  - ldp—Displays the best LDP tunnel routes in the routing table
  - local—Displays the best locally connected routes in the routing table
  - mbgp—Displays the best MBGP routes in the routing table
  - ospf—Displays the best OSPF routes owned by in the routing table
  - other—Displays the best internal control routes in the routing table
  - rip—Displays the best RIP routes in the routing table
  - rsvp—Displays the best RSVP tunnel routes in the routing table
  - static—Displays the best static routes added by network management to the routing table
  - static-rpf—Displays the best static RPF routes added by network management to the routing table
- filter—See Filtering show Commands
- summary—Displays summary counters for all routes in the IPv6 routing table

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]