> - radius pppoe nas-port-format unique

> # radius pppoe nas-port-format unique

> #### Syntax

> [ no ] radius pppoe nas-port-format unique

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Allows the E-series RADIUS client to use a unique value for the NAS-Port attribute for subscribers on PPPoE interfaces. The router derives the unique value from the subscriber’s profileHandle. The no version restores the default value, determined by the interface.

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.