> - radius include

> # radius include

> #### Syntax

> radius include attributeName
> { access-request | acct-on | acct-off | acct-start | acct-stop } { enable | disable }

> no radius include attributeName
> { access-request | acct-on | acct-off | acct-start | acct-stop }

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.
> l2c-access-loop-parameters attribute added in JUNOSe Release 7.2.0.
> l2cd attributes added in JUNOSe Release 9,0.0.
> framed-interface-id and framed-ipv6-prefix attributes, and acct-stop support for framed-ip-addr attribute added in JUNOSe Release 9.0.0.
> downstream-calculated-qos-rate and upstream-calculated-qos-rate attributes added in JUNOSe Release 9.1.0.

> #### Description

> Configures the inclusion of RADIUS attributes in RADIUS messages. Not all attributes are available in all message types. The listed attributes are included by default except where noted. The no version restores the default.

> #### Options

> - attributeName—One of the following RADIUS attributes; not all attributes are available in all message types.

>   Attributes available for Access-Request, Acct-Start, and Acct-Stop messages:

>   - acct-multi-session-id—Includes RADIUS attribute 50, Acct-Multi-Session-Id
>   - acct-tunnel-connection—Includes RADIUS attribute 68, Acct-Tunnel-Connection
>   - ascend-num-in-multilink—Includes RADIUS attribute 188, Ascend-Num-In-Multilink
>   - called-station-id—Includes RADIUS attribute 30, Called-Station-Id
>   - calling-station-id—Includes RADIUS attribute 31, Calling-Station-Id
>   - connect-info—Includes RADIUS attribute 77, Connect-Info
>   - dhcp-options—Includes RADIUS attribute 26-55, DHCP-Options
>   - dhcp-gi-address—Includes RADIUS attribute 26-57, DHCP-GI-Address
>   - dhcp-mac-address—Includes RADIUS attribute 26-56, DHCP-MAC Address
>   - downstream-calculated-qos-rate—Includes RADIUS attribute 26-141, Downstream-Calculated-Qos-Rate
>   - framed-interface-id—Excluded by default; includes RADIUS attribute 96, Framed-Interface-Id, if an IPv6 interface ID is assigned to the subscriber
>   - framed-ip-addr—Includes RADIUS attribute 8, Framed-IP-Address, if an IP address is assigned to the subscriber
>   - framed-ipv6-prefix—Excluded by default; includes RADIUS attribute 97, Framed-Ipv6-Prefix, if at least one IPv6 prefix is assigned to the subscriber
>   - interface-description—Includes RADIUS attribute 26-63, Interface-Desc
>   - l2c-downstream-data—Includes RADIUS attribute 26-92, L2C-Down-Stream-Data
>   - l2c-upstream-data—Includes RADIUS attribute 26-93, L2C-Up-Stream-Data
>   - l2c-upstream-data—Includes RADIUS attribute 26-93, L2C-Up-Stream-Data
>   - l2cd-acc-loop-cir-id—Excluded by default; includes RADIUS attribute 26-110, Acc-Loop-Cir-Id
>   - l2cd-acc-aggr-cir-id-bib—Excluded by default; includes RADIUS attribute 26-111, Acc-Aggr-Cir-Id-Bin
>   - l2cd-acc-aggr-cir-id-asc—Excluded by default; includes RADIUS attribute 26-112, Acc-Aggr-Cir-Id-Asc
>   - l2cd-act-data-rate-up—Excluded by default; includes RADIUS attribute 26-113, Act-Data-Rate-Up
>   - l2cd-act-data-rate-dn—Excluded by default; includes RADIUS attribute 26-114, Act-Data-Rate-Dn
>   - l2cd-min-data-rate-up—Excluded by default; includes RADIUS attribute 26-115, Min-Data-Rate-Up
>   - l2cd-min-data-rate-dn—Excluded by default; includes RADIUS attribute 26-116, Min-Data-Rate-Dn
>   - l2cd-att-data-rate-up—Excluded by default; includes RADIUS attribute 26-117, Att-Data-Rate-Up
>   - l2cd-att-data-rate-dn—Excluded by default; includes RADIUS attribute 26-118, Att-Data-Rate-Dn
>   - l2cd-max-data-rate-up—Excluded by default; includes RADIUS attribute 26-119, Max-Data-Rate-Up
>   - l2cd-max-data-rate-dn—Excluded by default; includes RADIUS attribute 26-120, Max-Data-Rate-Dn
>   - l2cd-min-lp-data-rate-up—Excluded by default; includes RADIUS attribute 26-121, Min-LP-Data-Rate-Up
>   - l2cd-min-lp-data-rate-dn—Excluded by default; includes RADIUS attribute 26-122, Min-LP-Data-Rate-Dn
>   - l2cd-max-interlv-delay-up—Excluded by default; includes RADIUS attribute 26-123, Max-Interlv-Delay-Up
>   - l2cd-act-interlv-delay-up—Excluded by default; includes RADIUS attribute 26-124, Act-Interlv-Delay-Up
>   - l2cd-max-interlv-delay-dn—Excluded by default; includes RADIUS attribute 26-125, Max-Interlv-Delay-Dn
>   - l2cd-act-interlv-delay-dn—Excluded by default; includes RADIUS attribute 26-126, Act-Interlv-Delay-Dn
>   - l2cd-dsl-line-state—Excluded by default; includes RADIUS attribute 26-127, DSL-Line-State
>   - l2cd-dsl-type—Excluded by default; includes RADIUS attribute 26-128, DSL-Type
>   - mlppp-bundle-name—Excluded by default; includes RADIUS attribute 26-62, MLPPP-Bundle-Name
>   - nas-port—Includes RADIUS attribute 5, NAS-Port
>   - nas-port-id—Includes RADIUS attribute 87, NAS-Port-Id
>   - nas-port-type—Includes RADIUS attribute 61, NAS-Port-Type
>   - pppoe-description—Includes RADIUS attribute 26-24, Pppoe-Description
>   - profile-service-description—Includes RADIUS attribute 26-53, Service-Description
>   - tunnel-client-auth-id—Includes RADIUS attribute 90, Tunnel-Client-Auth-Id
>   - tunnel-client-endpoint—Includes RADIUS attribute 66, Tunnel-Client-Endpoint
>   - tunnel-interface-id—Excluded by default; includes RADIUS attribute 26-44, Tunnel-Interface-ID
>   - tunnel-medium-type—Includes RADIUS attribute 65, Tunnel-Medium-Type
>   - tunnel-server-attributes—Excluded by default; includes all supported tunnel server attributes; that is, the attributes of the tunnel client when PPP is terminated at the LNS on the router
>   - tunnel-server-auth-id—Includes RADIUS attribute 91, Tunnel-Server-Auth-Id
>   - tunnel-server-endpoint—Includes RADIUS attribute 67, Tunnel-Server-Endpoint
>   - tunnel-type—Includes RADIUS attribute 64, Tunnel-Type
>   - upstream-calculated-qos-rate—Includes RADIUS attribute 26-142, Upstream-Calculated-Qos-Rate

>   Attributes available for Access-Request messages only:

>   - access-loop-parameters—Includes RADIUS attribute 26-81, L2c-Information

>   Attributes available for Acct-Start and Acct-Stop messages only:

>   - acct-link-count—Includes RADIUS attribute 51, Acct-Link-Count
>   - class—Includes RADIUS attribute 25, Class
>   - egress-policy-name—Includes RADIUS attribute 26-11, Egress-Policy-Name
>   - framed-compression—Includes RADIUS attribute 13, Framed-Compression
>   - framed-ip-netmask—Includes RADIUS attribute 9, Framed-IP-Netmask
>   - ingress-policy-name—Includes RADIUS attribute 26-10, Ingress-Policy-Name
>   - tunnel-assignment-id—Includes RADIUS attribute 82, Tunnel-Assignment-Id
>   - tunnel-preference—Includes RADIUS attribute 83, Tunnel-Preference

>   Attributes available for Acct-Stop messages only:

>   - input-gigapkts—Includes RADIUS attribute 26-35, Acct-Input-Gigapackets
>   - input-gigawords—Includes RADIUS attribute 52, Acct-Input-Gigawords
>   - l2tp-ppp-disconnect-cause—Includes RADIUS attribute 26-51, Disconnect-Cause
>   - output-gigapkts—Includes RADIUS attribute 26-36, Acct-Output-Gigapackets
>   - output-gigawords—Includes RADIUS attribute 53, Acct-Output-Gigawords

>   Attributes available for Access-Request, Acct-Start, Acct-Stop, Acct-On, and Acct-Off messages:

>   - nas-identifier—Includes RADIUS attribute 32, NAS-Identifier

>   Attributes available for Access-Request, Acct-On, and Acct-Off messages:

>   - acct-session-id—Includes RADIUS attribute 44, Acct-Session-Id

>   Attributes available for Acct-Start, Acct-Stop, Acct-On, and Acct-Off messages:

>   - event-timestamp—Includes RADIUS attribute 55, Event-Timestamp

>   Attributes available for Acct-On and Acct-Off messages only:

>   - acct-authentic—Includes RADIUS attribute 45, Acct-Authentic
>   - acct-delay-time—Includes RADIUS attribute 41, Acct-Delay-Time

>   Attributes available for Acct-Off messages only:

>   - acct-terminate-cause—Includes RADIUS attribute 49, Acct-Terminate-Cause
> - access-request—Specifies RADIUS Access-Request messages
> - acct-on—Specifies RADIUS Acct-On messages
> - acct-off—Specifies RADIUS Acct-Off messages
> - acct-start—Specifies RADIUS Acct-Start messages
> - acct-stop—Specifies RADIUS Acct-Stop messages
> - enable—Enables attribute inclusion
> - disable—Disables attribute inclusion; the attribute is excluded

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.