> - nas-port-type atm

> # nas-port-type atm

> #### Syntax

> nas-port-type atm { adsl-cap | adsl-dmt | idsl | sdsl | xdsl | cable | wireless-80211 |
> wireless-cdma | wireless-umts | wireless-1x-ev | wireless-other | iapp | value }

> no nas-port-type atm

> #### Release Information

> Command introduced before Release 7.1.0.

> #### Description

> Specifies the RADIUS NAS-Port-Type attribute (61) used for ATM interfaces. The no version removes the NAS-Port-Type setting.

> #### Options

> - adsl-cap—Asymmetric DSL, Carrierless Amplitude Phase Modulation
> - adsl-dmt—Asymmetric DSL, Discrete Multi-Tone
> - idsl—ISDN DSL
> - sdsl—Symmetric DSL
> - xdsl—DSL of unknown type
> - cable—Cable
> - wireless-80211—Wireless 802.11
> - wireless-cdma—Wireless code division multiple access (CDMA)
> - wireless-umts—Wireless universal mobile telecommunications system (UMTS)
> - wireless-1x-ev—Wireless 1xEV
> - wireless-other—Wireless other
> - iapp—Inter Access Point Protocol (IAPP)
> - value—Number in the range 0–65535

> #### Mode

> AAA Profile Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.