[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring RSVP-TE Profiles and MPLS Tunnel Profiles

Purpose

Display a specific RSVP-TE or tunnel profile, or all RSVP-TE or tunnel profiles.

Action

To display the default RSVP-TE profile:

    host1:pe2#show mpls rsvp profile default
    RSVP profile default: used by 0 interfaces
        refresh period: 30000 ms
        timeout factor: 3

To display all MPLS tunnel profiles:

    host1#show mpls tunnels profile
    MPLS Tunnel Profile tunnelProfile
      LSP setup using rsvp-te
      tunnel not announced to any IGP
      (Global) Retry forever
           at (Global) interval 5 during Lsp setup if there is route
      (Global) Retry forever
           at (Global) interval 5 during Lsp setup if there is no route
      metric is relative 0
      path option 2
        path to be dynamically calculated by isis
      destinations include: 1.1.1.1 2.2.2.2 3.3.3.3
        ISIS Level 2 routers
        OSPF border routers

Meaning

Table 50 lists the show mpls profile command output fields.

Table 50: show mpls profile Output Fields

Field Name | Field Description
--- | ---
profile | Number of interfaces that use the profile
refresh-period | Timeout period in seconds between generation of refresh messages
timeout factor | Number of refresh messages that can be lost before the session is ended

#### Related Topics

- show mpls profile

[Contents] [Prev] [Next] [Index] [Report an Error]