> - minimum-links
> - Related Topics
> - Configuring 802.3ad Link Aggregation and Link Redundancy in the JUNOSe Link Layer Configuration Guide

> # minimum-links

> #### Syntax

> minimum-links minimumLinkValue

> no minimum-links

> #### Release Information

> Command introduced in JUNOSe Release 10.0.0.

> #### Description

> Configures the minimum number of member links in the link aggregation group (LAG) bundle that must be in the Collecting/Distributing state for the LAG interface to be considered up. The no version resets the minimum number of member links to the default value.

> #### Options

> - minimumLinkValue—Minimum number of links in the LAG bundle in the range 1-8 (8 is the maximum number of member links per LAG bundle); default value is 1.

> #### Mode

> Interface Configuration

> #### Updated: 2009-04-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.