[Contents] [Prev] [Next] [Index] [Report an Error]

## Packet-Mirroring Terms

Table 46 defines terms used in this discussion of packet mirroring.

Table 46: Packet-Mirroring Terminology

Term | Meaning
--- | ---
Analyzer device | Device that receives the mirrored traffic from the E Series router. Also called the mediation device.
Analyzer interface | IP interface in analyzer mode on the E Series router that is used to direct mirrored traffic to the analyzer device.
CLI access class | Security level that grants access to specific CLI commands.
Mediation device | Device that receives the mirrored traffic from the E Series router. Also called the analyzer device.
Mirrored interface | Statically or dynamically configured interface on which traffic is being mirrored.
Mirrored user | User whose traffic is being mirrored.
Requesting authority | Group that is authorized to request or conduct packet mirroring.
Salt encryption | Random string of data used to modify a password hash.
Secure policy | Policies created with a mirror action and that contain information about where to forward mirrored traffic.
Trigger | RADIUS attribute that identifies a user whose traffic is to be mirrored. Packet mirroring starts when a trigger is detected. An E Series router supports a maximum of 100 mirror trigger rules.

[Contents] [Prev] [Next] [Index] [Report an Error]