[Contents] [Prev] [Next] [Index] [Report an Error]

# baseline ip dhcp-local

#### Syntax

baseline ip dhcp-local [ interface interfaceType interfaceSpecifier ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets a baseline for DHCP local server statistics. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved. There is no no version.

#### Options

- interfaceType—One of the following interface types listed in Interface Types and Specifiers
  - atm
  - fastEthernet
  - gigabitEthernet
  - tenGigabitEthernet
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]