[Contents] [Prev] [Next] [Index] [Report an Error]

## Index

A B C D E F G H I J L M N P Q R S T U V

A

> access lists, IP
>   specifying multicast groups 1
> access lists, IPv6
>   specifying multicast groups 1
> advertising DVMRP routes 1, 2
> assert messages 1
> assigning multicast groups 1, 2
> auto-RP router
>   PIM sparse mode 1
>   PIM sparse-dense mode 1

B

> baseline commands
>   baseline ip dvmrp 1
>   baseline ip igmp 1
>   baseline ip igmp-proxy interface 1
>   baseline ipv6 mld 1
>   baseline ipv6 mld-proxy interface 1
> BFD (Bidirectional Forwarding Detection)
>   RIP, configuring for 1, 2
> BGP multicasting 1, 2

C

> Class D IPv4 addresses 1
> clear ip commands
>   clear ip dvmrp route 1
>   clear ip mroute 1, 2
>   clear ip pim auto-rp 1
>   clear ip pim interface count 1, 2
>   clear ip pim remote-neighbor count 1
> clear ipv6 commands
>   clear ipv6 mroute 1
>   clear ipv6 pim remote-neighbor count 1
> conventions
>   notice icons 1
>   text and syntax 1
> customer support 1
>   contacting JTAC 1

D

> data MDT, creating 1
> data path failure
>   detecting RIP 1, 2
> debug commands
>   debug ip pim 1
>   debug ipv6 pim 1
> default MDT, creating 1
> detecting RIP data path failure 1, 2
> disable command 1
> disable-dynamic-redistribute command
>   DVMRP 1
> disabling dynamic route redistribution
>   DVMRP 1
> Distance Vector Multicast Routing Protocol. See DVMRP
> documentation set
>   comments on 1
> downstream interface 1, 2
> DRs (designated routers)
>   PIM routing 1, 2
> DVMRP (Distance Vector Multicast Routing Protocol)
>   advertising routes 1, 2
>   configuring
>     limits 1
>     summary addresses 1
>   default router, configuring 1
>   deleting routes 1
>   enabling
>     on a virtual router 1
>     on an interface 1
>   exchanging unicast routes 1
>   filtering reports 1
>   metric 1
>   monitoring 1
>   neighbors 1
>   overview 1
>   pruning 1
>   summary addresses 1
>   tunnels 1
>   using with IGMP 1
>   using with PIM 1, 2
> dynamic route redistribution, disabling
>   in DVMRP 1

E

> encapsulation commands
>   encapsulation vlan 1, 2
> exchanging DVMRP unicast routes 1

F

> filtering
>   DVMRP reports 1

G

> group membership
>   queries 1, 2
>   reports 1, 2

H

> hardware multicast packet replication
>   monitoring 1, 2
>   OIF mapping 1, 2
>   overview 1, 2
> hello interval 1, 2
>   PIM 1, 2, 3, 4, 5, 6, 7, 8, 9
> hold time
>   PIM sparse mode 1
> hop count 1

I

> IGMP (Internet Group Management Protocol) 1
>   configuring 1
>   disabling 1, 2
>   enabling 1, 2
>   limiting groups on interfaces 1
>   monitoring 1, 2
>   performing host functions 1
>   querier 1
>   removing 1
>   specifying version 1, 2, 3
> igmp commands
>   igmp disable 1
>   igmp promiscuous 1
> IGMP proxy 1
>   configuring 1
>   enabling 1
>   monitoring 1
>   version 1
> IGMP reports, accepting 1
> IGP (interior gateway protocol) 1
> importing routes. See redistributing routes
> Internet Group Management Protocol. See IGMP
> investigating IP multicast routes 1
> IP addresses
>   class D 1
>   for multicasting 1
> ip commands
>   ip block-multicast-sources 1
>   ip multicast-routing 1, 2, 3
>   ip multicast-routing disable-rpf-check 1, 2
>   ip multicast-routing permanent-mroute 1
>   ip route-type 1
>   ip rpf-route 1
>   ip unnumbered 1, 2
>   mroute port limit 1, 2, 3, 4
> ip dvmrp commands 1
>   ip dvmrp 1, 2
>   ip dvmrp accept-filter 1
>   ip dvmrp announce-list 1
>   ip dvmrp auto-summary 1
>   ip dvmrp disable 1
>   ip dvmrp metric-offset 1
>   ip dvmrp route-limit 1
>   ip dvmrp routehog-notification 1
>   ip dvmrp summary-address 1
>   ip dvmrp unicast-routing 1
>   See also show ip dvmrp commands
> ip igmp commands 1
>   ip igmp 1
>   ip igmp access-group 1
>   ip igmp access-source-group 1, 2, 3
>   ip igmp group limit 1
>   ip igmp immediate-leave 1
>   ip igmp last-member query-interval 1
>   ip igmp promiscuous 1
>   ip igmp querier 1
>   ip igmp querier-timeout 1
>   ip igmp query-interval 1
>   ip igmp query-max-response-time 1
>   ip igmp robustness 1
>   ip igmp ssm-map enable 1
>   ip igmp ssm-map static 1
>   ip igmp static-exclude 1
>   ip igmp static-group 1
>   ip igmp static-include 1
>   ip igmp version 1, 2, 3
>   ip igmp-proxy 1
>   ip igmp-proxy unsolicited-report-interval 1
>   ip igmp-proxy V1-router-present-time 1
>   See also show ip igmp commands
> ip multicast commands
>   ip multicast admission-bandwidth-limit 1
>   ip multicast ioa-packet-replication 1
>   ip multicast-routing bandwidth-map 1
> IP multicast groups
>   assigning to an interface 1
>   identifying 1
>   leaving 1
>   maintaining membership of 1
>   reporting 1
>   specifying 1
> IP multicast interfaces, monitoring 1
> IP multicast routes 1
> IP multicasting
>   benefits of 1
>   deleting routes 1
>   enabling 1
>   M-BONE 1
>   monitoring 1
> ip pim commands 1
>   ip pim 1
>   ip pim bsr-candidate 1
>   ip pim data-mdt 1
>   ip pim group-address-pool 1
>   ip pim join-filter 1
>   ip pim query-interval 1
>   ip pim rp-address 1
>   ip pim rp-candidate 1
>   ip pim send-rp-announce 1
>   ip pim send-rp-discovery scope 1
>   ip pim sparse-mode graceful-restart-duration 1
>   ip pim spt-threshold 1
>   See also show ip pim commands
> ip rip commands
>   ip rip bfd-liveness-detection 1, 2
> IP tunnels
>   monitoring 1
> ipv6 commands 1
>   ip route-type 1
>   ipv6 block-multicast-sources 1
>   ipv6 mld robustness 1
>   ipv6 multicast-routing 1
>   ipv6 multicast-routing disable-rpf-check 1
>   ipv6 multicast-routing permanent-route 1
>   ipv6 rpf-route 1
>   See also show ipv6 commands
> ipv6 mld commands 1
>   ipv6 mld 1
>   ipv6 mld access-group 1
>   ipv6 mld access-source-group 1
>   ipv6 mld apply-oif-map 1
>   ipv6 mld explicit-tracking 1
>   ipv6 mld group limit 1
>   ipv6 mld immediate-leave 1
>   ipv6 mld last-member query-interval 1
>   ipv6 mld oif-map 1
>   ipv6 mld querier-timeout 1
>   ipv6 mld query-interval 1
>   ipv6 mld query-max-response-time 1
>   ipv6 mld ssm-map enable 1
>   ipv6 mld ssm-map static 1
>   ipv6 mld static-exclude 1
>   ipv6 mld static-group 1
>   ipv6 mld static-include 1
>   ipv6 mld version 1, 2, 3
>   ipv6 mld-proxy 1
>   ipv6 mld-proxy unsolicited-report-interval 1
>   ipv6 mld-proxy version 1
>   See also show ipv6 mld commands
> IPv6 multicast
>   benefits of 1
>   deleting routes 1
>   enabling 1
>   monitoring 1
> ipv6 multicast commands
>   ipv6 multicast admission-bandwidth-limit 1
>   ipv6 multicast ioa-packet-replication 1
>   ipv6 multicast-routing bandwidth-map 1
> IPv6 multicast groups
>   assigning to an interface 1
>   identifying 1
>   leaving 1
>   maintaining membership of 1
>   reporting 1
>   specifying 1
> ipv6 pim commands 1, 2
>   ipv6 pim 1
>   ipv6 pim bsr-candidate 1
>   ipv6 pim join-filter 1
>   ipv6 pim query-interval 1
>   ipv6 pim rp-address 1
>   ipv6 pim rp-candidate 1
>   ipv6 pim spt-threshold 1
>   See also show ipv6 pim commands

J

> join messages 1, 2

L

> leave group membership messages 1, 2
> leaving an IP multicast group 1
> leaving an IPv6 multicast group 1
> limiting IGMP groups on interfaces 1
> limiting MLD groups on interfaces 1
> liveness detection
>   RIP and BFD 1, 2

M

> M-BONE (multicast backbone of the Internet) 1
> manuals
>   comments on 1
> MDT (Multicast Distribution Tree)
>   creating with default MDT 1
> mdt commands
>   mdt-data-delay 1
>   mdt-data-holddown 1
>   mdt-data-timeout 1
>   mdt-interval 1
> metric
>   DVMRP 1
> MLD (Multicast Listener Discovery) 1
>   configuring 1
>   disabling 1, 2
>   enabling 1, 2
>   limiting groups on interfaces 1
>   monitoring 1
>   performing host functions 1
>   removing 1
>   specifying version 1, 2
> mld disable command 1
> MLD proxy 1
>   configuring 1
>   enabling 1
>   monitoring 1
>   version 1
> mrinfo requests, support for 1
> mtrace command 1
> multicast
>   IP. See IP multicasting
>   IPv6. See IPv6 multicast
> Multicast Distribution Tree. See MDT
> multicast group port limit command 1, 2
> Multicast Listener Discovery. See MLD
> multicast VPNs
>   creating with data MDTs 1
>   creating with the default MDT 1
>   overview 1

N

> neighbors, DVMRP 1
> notice icons 1

P

> PIM (Protocol Independent Multicast) 1, 2, 3
>   displaying events 1, 2
>   enabling
>     on a virtual router 1, 2
>     on an interface 1, 2
>   monitoring 1, 2, 3, 4
>   removing 1, 2
>   resetting counters and mappings 1, 2
>   using with DVMRP 1, 2
>   using with IGMP 1
>   using with MLD 1
>   See also PIM dense mode, PIM sparse mode, PIM sparse-dense mode
> PIM dense mode 1, 2
>   See also PIM
> pim disable command 1, 2
> PIM SM. See PIM sparse mode
> PIM sparse mode 1, 2
>   configuring auto-RP router 1
>   joining groups 1
>   pruning 1
>   remote neighbors, configuring 1, 2, 3, 4
>   setting a threshold 1, 2
>   timers 1, 2
> PIM sparse-dense mode 1
>   configuring auto-RP router 1
>   overview 1
> PIM SSM (PIM source-specific multicast)
>   enabling 1, 2
>   requirements for IGMPv3 1
>   requirements for MLDv2 1
> Protocol Independent Multicast. See PIM
> prune messages 1, 2

Q

> query-interval command 1

R

> reachability commands
>   IP multicast 1
> redistribute command
>   DVMRP 1
> redistributing routes, DVMRP 1
> redistribution routes
>   disabling dynamic (DVMRP) 1
> remote neighbors
>   PIM sparse mode
>     configuring 1, 2, 3, 4
> remote-neighbor command 1
> removing PIM 1, 2
> rendezvous point router. See RP routers
> reporting IP multicast groups 1
> reporting IPv6 multicast groups 1
> resetting PIM counters and mappings 1, 2
> reverse-path forwarding. See RPF
> RIP (Routing Information Protocol)
>   BFD liveness detection and 1, 2
>   detecting path failures 1, 2
>   purging learned routes 1, 2
> route-map command 1
> router commands
>   router dvmrp 1, 2
>   router igmp 1
>   router mld 1
>   router pim 1, 2, 3, 4
> routes
>   using for other protocols 1, 2
> routing policy commands
>   set admission-bandwidth 1
>   set qos-bandwidth 1
> RP (rendezvous point) routers 1, 2
>   assigning automatically 1
>   configuring
>     automatic 1, 2
>     static 1, 2
> RPF (reverse-path forwarding) 1, 2, 3
> RPF routes, monitoring 1, 2

S

> set threshold command 1
> setting
>   baseline
>     DVMRP 1
>     IGMP 1
>     IGMP Proxy 1
>     MLD 1
>     MLD Proxy 1
>   DVMRP hop-count 1
>   PIM SPT threshold
>     IP 1
>     IPv6 1
> shared trees 1, 2, 3, 4
> shortest path trees. See SRTs
> show ip commands
>   show ip mroute 1
>   show ip mroute count 1, 2, 3, 4
>   show ip mroute summary 1
>   show ip rpf-route 1
> show ip dvmrp commands
>   show ip dvmrp 1
>   show ip dvmrp interface 1
>   show ip dvmrp mroute 1
>   show ip dvmrp neighbor 1
>   show ip dvmrp route 1
>   show ip dvmrp routeNextHop 1
> show ip igmp commands
>   show ip igmp 1
>   show ip igmp groups 1
>   show ip igmp interface 1
>   show ip igmp interface brief 1
>   show ip igmp membership 1
>   show ip igmp-proxy 1
>   show ip igmp-proxy groups 1
>   show ip igmp-proxy interface 1
> show ip multicast commands
>   show ip multicast protocols 1
>   show ip multicast protocols brief 1
>   show ip multicast routing 1
> show ip pim commands
>   show ip pim 1
>   show ip pim auto-rp 1
>   show ip pim bsr 1
>   show ip pim data-mdt 1
>   show ip pim dense-mode sg-state 1
>   show ip pim interface 1
>   show ip pim neighbor 1
>   show ip pim rp 1
>   show ip pim rp-hash 1
>   show ip pim sparse-mode sg-state 1
>   show ip pim sparse-mode unicast-route 1
>   show ip pim spt-threshold 1
> show ipv6 commands
>   show ipv6 mroute 1
>   show ipv6 mroute count 1, 2
>   show ipv6 mroute summary 1
>   show ipv6 rpf-route 1
> show ipv6 mld commands
>   show ipv6 mld 1
>   show ipv6 mld groups 1
>   show ipv6 mld interface 1
>   show ipv6 mld interface brief 1
>   show ipv6 mld membership 1
>   show ipv6 mld-proxy 1
>   show ipv6 mld-proxy groups 1
>   show ipv6 mld-proxy interface 1
> show ipv6 mld ssm-mapping command 1
> show ipv6 multicast commands
>   show ipv6 multicast protocols 1
>   show ipv6 multicast protocols brief 1
>   show ipv6 multicast routing 1
> show ipv6 pim commands
>   show ipv6 pim 1
>   show ipv6 pim bsr 1
>   show ipv6 pim interface 1
>   show ipv6 pim neighbor 1
>   show ipv6 pim remote-neighbor 1
>   show ipv6 pim rp 1
>   show ipv6 pim rp-hash 1
>   show ipv6 pim sparse-mode sg-state 1
>   show ipv6 pim sparse-mode unicast-route 1
>   show ipv6 pim spt-threshold 1
> show multicast group limit command 1, 2
> source-rooted trees. See SRTs
> Source-Specific Multicast for IP—draft-ietf-ssm-arch-06.txt (March 2005 expiration) 1
> specifying IP multicast groups 1
> specifying IPv6 multicast groups 1
> SPTs (shortest path trees). See SRTs
> SRTs (source-rooted trees) 1, 2, 3, 4, 5
> static routes
>   configuring 1, 2
> summary addresses
>   DVMRP routing 1
> support, technical See technical support

T

> technical support
>   contacting JTAC 1
> text and syntax conventions 1
> timers
>   PIM sparse mode 1, 2
> trace packets 1
> tunnel group-address-pool command 1
> tunnel mdt command 1

U

> undebug commands
>   undebug ip pim 1
>   undebug ipv6 pim 1
> unicast routes, DVMRP 1
> update-source command 1
> upstream interface 1, 2

V

> vlan commands
>   encapsulation vlan 1, 2

[Contents] [Prev] [Next] [Index] [Report an Error]