> - diag-level

> # diag-level

> #### Syntax

> diag-level [ normal ] [ bypass ]

> #### Release Information

> Command introduced in JUNOSe Release 9.2.0.

> #### Description

> Sets the diagnostics level on the active or standby SRP module to reduce boot time during a cold and a warm boot. The default diagnostics level is normal. There is no no version.

> #### Options

> - normal—executes full diagnostics on the boot of the line card

>   bypass—skips diagnostic tests on the boot of the line card

> #### Mode

> Global Configuration

> #### Updated: 2009-04-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.