[Contents] [Prev] [Next] [Report an Error]

# 10GE PR IOA

> IOA label | ES2-S2 10GE PR IOA
> Number of IOA ports | 2 1 active, 1 redundant
> Software release | First supported: 7.2.0
> Description | 40 W Full-height module Uses a range of 10-gigabit small form-factor pluggable (XFP) transceivers to support different modes and cable lengths. Pairs only with ES2 10G UPLINK LM, ES2 10G LM, and ES2 10G ADV LM to provide 10-Gigabit Ethernet operation through a single line interface In a 100 Gbps configuration, the E320 router can accommodate up to two ES2 10G UPLINK LM and ES2-S2 10GE PR IOA combinations. You must install a combination in either of the turbo slots (slot 2 or slot 4). In a 100 Gbps configuration, the E320 router can accommodate up to two ES2 10G LM and ES2-S2 10GE PR IOA combinations In a 120 Gbps configuration, the E120 router can accommodate up to six ES2 10G UPLINK LM and ES2-S2 10GE PR IOA combinations. You can install a combination in any of the line module slots. In a 320 Gbps configuration, the E320 router can accommodate up to twelve ES2 10G UPLINK LM and ES2-S2 10GE PR IOA combinations. You can install a combination in any of the line module slots. In a 320 Gbps configuration, the E320 router can accommodate up to twelve ES2 10G LM and ES2-S2 10GE PR IOA combinations
> Capability | Ethernet (IEEE 802.3ae) 10Gb Base-SR/LR/ER/ZR Port can operate in full duplex mode with an average data rate of 10 Gbps
> Software features | See Ethernet IOAs for information about the layer 2 and layer 3 protocols and applications that this module combination supports.
> Model compatibility | E320 router E120 router
> Line module compatibility | ES2 10G UPLINK LM ES2 10G LM ES2 10G ADV LM
> SRP module compatibility | SRP-100 SRP-120 SRP-320
> Line module redundancy compatibility | Not applicable
> Port redundancy support | Yes
> Cables and connectors (multimode [SR]) | One LC full duplex connector Transmit power: min: –7.3 dBm max: –1.0 dBm Receive input power: min: –9.9 dBm max: –1.0 dBm See the following corresponding table (SR Fiber Optic Cabling) for cabling requirements. See E120 and E320 Hardware Guide, Chapter 5, Cabling the Router for more information.
> Cables and connectors (single-mode [LR]) | One LC full duplex connector Transmit power: min: –8.2 dBm max: 0.5 dBm Receive input power: min: –14.4 dBm max: 0.5 dBm See the following corresponding table (LR Fiber Optic Cabling) for cabling requirements. See E120 and E320 Hardware Guide, Chapter 5, Cabling the Router for more information.
> Cables and connectors (single-mode [ER]) | One LC full duplex connector Transmit power: min: –4.7 dBm max: 4.0 dBm Receive input power: min: –15.8 dBm max: –1.0 dBm See the following corresponding table (ER Fiber Optic Cabling) for cabling requirements. See E120 and E320 Hardware Guide, Chapter 5, Cabling the Router for more information.
> Cables and connectors (single-mode [ZR]) | One LC full duplex connector Transmit power: min: 0 dBm max: 4 dBm Receive input power: min: –24.0 dBm max: –7.0 dBm See the following corresponding table (ZR Fiber Optic Cabling) for cabling requirements. See E120 and E320 Hardware Guide, Chapter 5, Cabling the Router for more information.
> LEDs | Board-level LEDs: OK (green)—IOA online and is functioning properly FAIL (red)—Failure detected Port LEDs: LK (green)—Ethernet link is up ACT (green)—Blinks when Ethernet traffic is being received Port labels: W—Working port P—Protect port (LK blinks when active cable is attached even though it is not the active working port)
> Alarms, errors, and events | See Monitoring Ethernet Interfaces in JUNOSe Physical Layer Configuration Guide, Chapter 5, Configuring Ethernet Interfaces.

> Table 21: SR Fiber Optic Cabling

> Fiber Type | Minimal Modal Bandwidth at 850 nm (MHz*km) | Maximum Operating Range (meters)
> --- | --- | ---
> 62.5 microns | 160 | 26 (85.3 ft)
> | 200 | 33 (108.27 ft)
> 50 microns | 400 | 66 (216.54 ft)
> | 500 | 82 (269.03 ft)
> | 2000 | 300 (984.25 ft)

> Table 22: LR Fiber Optic Cabling

> Fiber Type | Nominal Wavelength (nm) | Maximum Operating Range (kilometers)
> --- | --- | ---
> 9 microns | 1310 | 10 (6.2 miles)

> Table 23: ER Fiber Optic Cabling

> Fiber Type | Nominal Wavelength (nm) | Maximum Operating Range (kilometers)
> --- | --- | ---
> 9 microns | 1550 | 40 (24.85 miles)

> Table 24: ZR Fiber Optic Cabling

> Fiber Type | Nominal Wavelength (nm) | Maximum Operating Range (kilometers)
> --- | --- | ---
> 9 microns | 1550 | 80 (49.6 miles)

[Contents] [Prev] [Next] [Report an Error]