[Contents] [Prev] [Next] [Report an Error]

# GE 1000Base-SX Module Combination (1 Port) (128 MB)

This module combination is no longer supported because the line module has reached end-of-life. However, the I/O module is still supported.

> Line module label | GE/FE
> I/O module label | GE I/O SFP
> Number of I/O ports | 1 active, 1 redundant
> Software release | First supported: 2.0.0 Final supported: 5.2.x
> Description | 130 W Gigabit Ethernet The GE SFP I/O module uses a range of small form-factor pluggable (SFP) transceivers to support different modes and cable lengths. The transceivers on this GE I/O module are 1000Base-SX compliant.
> Type | ASIC
> Capability | Ethernet (IEEE 802.3z) 1000Base-SX
> Software features | See ERX Module Guide, Appendix A, Module Protocol Support for information about the layer 2 and layer 3 protocols and applications that this module combination supports.
> Model compatibility | ERX-7xx models ERX-14xx models ERX-310 router
> SRP module compatibility | SRP-5G+ SRP-10G SRP-40G SRP-40G PLUS SRP-SE10G
> Module redundancy support | Not applicable
> Cables and connectors | LC full duplex Tx power: min: –9.5 dBm max: –4 dBm Center wavelength: 850 nm Rx input power: min: –17 dBm max: –3 dBm Rated for 275 m (300 yards) over 62.5-micron core cable Rated for 550 m (601 yards) over 50-micron core cable See ERX Hardware Guide, Chapter 5, Cabling ERX Routers for more information.
> LEDs | See ERX Module Guide, Appendix B, Module LEDs.
> Alarms, errors, and events | See Monitoring Ethernet Interfaces in the Configuring Ethernet Interfaces chapter of the JUNOSe Physical Layer Configuration Guide for Release 8.0.x and earlier.

[Contents] [Prev] [Next] [Report an Error]