[Contents] [Prev] [Next] [Index] [Report an Error]

# show ldp binding

#### Syntax

For MPLS binding information:

show [ mpls ] ldp { [ ip ] binding | binding ip }
[ destAddr [ maskLength | maskAddress ] [ longer-prefixes ] ]
[ interface interfaceType interfaceSpecifier ]
[ neighbor ipAddress ] [ generic | atm ] [ local | remote ]
[ label { atm vpi vci | explicit-null-label | implicit-null-label |
labelNumber [ labelRangeEnd ] } ]
[ brief ] [ filter ]

For layer 2 over MPLS binding information:

show [ mpls ] ldp binding layer2-vc [ vc-type vcType [ vc-id vcId ] ]
[ interface interfaceType interfaceSpecifier ]
[ neighbor ipAddress ] [ generic | atm ] [ local | remote ]
[ label { atm vpi vci | explicit-null-label | implicit-null-label |
labelNumber [ labelRangeEnd ] } ]
[ brief ] [ filter ]

#### Release Information

Command introduced in JUNOSe Release 7.1.0.
explicit-null-label keyword and optional mpls keyword added in JUNOSe Release 7.2.0.

#### Description

Displays label bindings from the MPLS label information base. This command displays the same output as the show mpls binding command.

#### Options

- mpls—Specifies optional keyword for compatibility with non–E Series implementations
- ip—Specifies optional keyword for compatibility with non–E Series implementations when placed before the binding keyword; when present (either before or after this keyword) displays label binding information only for IP prefixes
- destAddr—Destination address for which you want information displayed; if not specified, displays all destinations
- maskLength—Prefix length for the destination address
- maskAddress—Address mask to be applied to the destination address
- longer-prefixes—Displays information for prefixes that are equal to or more specific than the specified prefix
- interface—Displays labels associated with the specified interface
  - interfaceType—Interface type; see Interface Types and Specifiers
  - interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- ipAddress—Displays labels associated with the specified neighbor
- generic—Displays only generic labels
- atm—Displays only ATM VPI/VCI labels
- local—Displays only local labels
- remote—Displays only remote labels
- atm—Displays the specified ATM VPI/VCI labels
  - vpi—Specifies ATM VPI that partially designates a label
  - vci —Specifies ATM VCI that partially designates a label
- explicit-null-label—Displays binding information for the explicit null label
- implicit-null-label—Displays binding information for the implicit null label
- labelNumber—Label for which binding information is displayed; number in the range 16–1048575
- labelRangeEnd—Label designating the high end of a range of labels for which binding information is specified; number in the range 16–1048575
- brief—Displays limited information
- filter—See Filtering show Commands
- layer2-vc—Displays binding information for layer 2 over MPLS
- vcType—One of the following types of virtual circuit over MPLS for which binding information is displayed: aal5-vcc, ethernet, frame-relay, vlan
- vcId—Virtual circuit identifier, number in the range 1–4294967295

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]