[Contents] [Prev] [Next] [Index] [Report an Error]

# ip rsvp bandwidth

#### Syntax

{ ip rsvp | mpls } bandwidth bandwidth

no { ip rsvp | mpls } bandwidth

#### Description

Specifies the total bandwidth reservable on the interface in a non–E Series implementation. See the mpls bandwidth command for a complete description and syntax.

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]