[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring PPPoE for Ethernet Modules

You can configure PPPoE on Fast Ethernet (FE), Gigabit Ethernet (GE), and 10-Gigabit Ethernet (10GE) modules. You can configure Ethernet interfaces with IP only, with PPPoE only, with both IP and PPPoE, and with or without VLANs.

This section provides information about configuring PPPoE without VLANs. If you want to configure PPPoE with VLANs, see Configuring VLAN and S-VLAN Subinterfaces , which shows common VLAN configurations such as:

- PPPoE over VLAN
- IP over VLAN and PPPoE over VLAN

  | Note: Configuring VLAN and S-VLAN Subinterfaces provides other non-VLAN configuration examples, such as configurations using MPLS.

For more information about specific Ethernet modules and the protocols and applications they support, see:

- ERX Module Guide, Appendix A, Module Protocol Support (for ERX7xx models, ERX14xx models, and ERX310 router)
- E120 and E320 Module Guide, Appendix A, IOA Protocol Support (for E120 and E320 routers)

## PPPoE Interface and Subinterface Limits

PPPoE subinterfaces can be distributed in any way across I/O module ports. For example, you can configure the maximum supported number of PPPoE subinterfaces on one port of an FE-2 I/O module and no PPPoE subinterfaces on the other port.

For information about current system maximums supported for PPPoE interfaces and subinterfaces, see JUNOSe Release Notes, Appendix A, System Maximums.

## Configuring PPPoE Without VLANs

To configure PPPoE over an Ethernet interface without VLANs:

1. Specify a Fast Ethernet, Gigabit Ethernet, or 10-Gigabit Ethernet interface.
   `
   host1(config)#interface fastEthernet 4/1
   `
2. Specify PPPoE as the encapsulation method on the interface.
   `
   host1(config-if)#pppoe
   `
3. Create a PPPoE subinterface.
   `
   host1(config-if)#pppoe subinterface fastEthernet 4/1.1
   `
4. Specify PPP as the encapsulation method on the interface.
   `
   host1(config-subif)#encapsulation ppp
   `
5. (Optional) Configure an access concentrator (AC) name on the PPPoE interface.
   `
   host1(config-subif)#pppoe acname CYM9876
   `
6. (Optional) Set up the router to prevent a client from establishing more than one session using the same MAC address.
   `
   host1(config-subif)#pppoe duplicate-protection
   `
7. Assign an IP address and mask.
   `
   host1(config-if)#ip address 192.6.129.5 255.255.255.0
   `
8. (Optional) Configure additional PPPoE subinterfaces by completing Steps 3 through 7 using unique numbering.

Figure 35 illustrates the interface stack for this configuration.

Figure 35: Example of PPPoE Stacking

encapsulation ppp

- Use to specify PPP as the encapsulation method for the interface.
- Example
  `
  host1(config-if)#encapsulation ppp
  `
- Use the no version to disable PPP on an interface.
- See encapsulation ppp.

interface fastEthernet

- Use to select a Fast Ethernet interface.
- For more information, see chapter Configuring Ethernet Interfaces in JUNOSe Physical Layer Configuration Guide.
- Example
  `
  host1(config)#interface fastEthernet 1/0
  `
- Use the no version to remove IP from an interface or subinterface. You must issue the no version from the highest level down; you cannot remove an interface or subinterface if the one above it still exists.
- See interface fastEthernet.

interface gigabitEthernet

interface tenGigabitEthernet

- Use to select a Gigabit Ethernet interface or a 10-Gigabit Ethernet interface.
- To specify a Gigabit Ethernet interface for ERX7xx models, ERX14xx models, and ERX310 router, use the slot/port[.subinterface ] format.
- To specify a Gigabit Ethernet interface or 10-Gigabit Ethernet interface for E120 and E320 routers, use the slot/adapter/port[.subinterface ] format.
- For more information, see chapter Configuring Ethernet Interfaces in JUNOSe Physical Layer Configuration Guide.
- Examples
  `
  host1(config)#interface gigabitEthernet 1/0
  host1(config)#interface gigabitEthernet 4/0/1 6.0.0FRS
  host1(config)#interface tenGigabitEthernet 4/0/1
  `
- Use the no version to remove IP from an interface. You must issue the no version from the highest level down; you cannot remove an interface or subinterface if the one above it still exists.
- See interface gigabitEthernet.
- See interface tenGigabitEthernet.

ip address

- Use to assign an IP address and subnet mask to an interface or subinterface.
- Example
  `
  host1(config-if)#ip address 192.1.1.1 255.255.255.0
  `
- Use the no version to remove an IP address or disable IP processing.
- See ip address.

pppoe

- Use to specify PPPoE as the encapsulation method for the interface.
- This command creates a PPPoE major interface.
- Example
  `
  host1(config-if)#pppoe
  `
- Use the no version to remove the PPPoE major interface.
- See pppoe.

pppoe acName

- Use to configure an access concentrator (AC) name on the PPPoE interface. When the AC (the server) receives a PPPoE Active Discovery Initiation (PADI) packet that it can serve, it replies by sending a PPPoE Active Discovery Offer (PADO) packet. The PADO packet contains the AC name configured using this command.
- If the AC name is not configured, the router name is used.
- The AC name can be a maximum of 64 characters.
- Example
  `
  host1(config-subif)#pppoe acName CYM9876
  `
- Use theno version to remove the AC name.
- See pppoe acName.

pppoe duplicate-protection

- Use to prevent a client from establishing more than one session using the same MAC address.
- This feature is disabled by default.
- Example
  `
  host1(config-subif)#pppoe duplicate-protection
  `
- Use the no version to disable duplicate protection.
- See pppoe duplicate-protection.

pppoe subinterface fastEthernet

- Use to create a PPPoE subinterface on a Fast Ethernet module.
- On ERX7xx models, ERX14xx models, and the ERX310 router, use the slot/port/pppoeSubinterface format.
- Example
  `
  host1(config)#pppoe subinterface fastEthernet 4/1.1
  `
- Use the no version to remove the PPPoE subinterface.
- See pppoe subinterface.

[Contents] [Prev] [Next] [Index] [Report an Error]