> - radius override nas-ip-addr tunnel-client-endpoint

> # radius override nas-ip-addr tunnel-client-endpoint

> #### Syntax

> radius override nas-ip-addr tunnel-client-endpoint

> no radius override nas-ip-addr

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Configures the RADIUS client (LNS) to override the standard use of the NAS-IP-Address [4] RADIUS attribute and instead use the tunnel-client-endpoint (LAC) IP address. The no version restores the default address.

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.