[Contents] [Prev] [Next] [Index] [Report an Error]

# aps force

#### Syntax

aps force channelNumber

no aps force

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Forces the specified interface to be replaced by the inactive interface in an APS/MSP group. The no version allows the specified interface to resume operation.

#### Options

- channelNumber—One of the following channel numbers:
  - 0—Switches from the protect interface back to the working interface
  - 1—Switches from the working interface to the protect interface

#### Mode

Controller Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]