> - radius remote-circuit-id-format

> # radius remote-circuit-id-format

> #### Syntax

> radius remote-circuit-id-format { [ nas-identifier ] { agent-circuit-id | agent-remote-id | agent-circuit-id agent-remote-id } | dsl-forum-1 }

> no radius remote-circuit-id format

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.
> dsl-forum-1 keyword added in JUNOSe Release 7.2.0.

> #### Description

> Specifies the format of the PPPoE remote circuit ID value sent from a DSLAM and captured on the router. You can format the PPPoE remote circuit ID value to include either or both of the agent-circuit-ID (suboption 1) and agent-remote-id (suboption 2) suboptions of the tags supplied by the PPPoE intermediate agent. The no version restores the default format, agent-circuit-id.

> #### Options

> - nas-identifier—Formats the PPPoE remote circuit ID value to include the NAS-Identifier [32] RADIUS attribute with either or both of the agent-circuit-id and agent-remote-id suboptions. If you include the nas-identifier keyword, you must also include either or both of the agent-circuit-id and agent-remote-id keywords.
> - agent-circuit-id—Formats the PPPoE remote circuit ID value to include only the agent-circuit-id suboption; this is the default format
> - agent-remote-id—Formats the PPPoE remote circuit ID value to include only the agent-remote-id suboption
> - agent-circuit-id agent-remote-id—Formats the PPPoE remote circuit ID value to include both the agent-circuit-id and agent-remote-id suboptions
> - dsl-forum-1—Formats the PPPoE remote circuit ID value to append the agent-circuit-id suboption value to an interface specifier that is consistent with the recommended format in the DSL Forum Technical Report (TR)-101—Migration to Ethernet-Based DSL Aggregation (April 2006).

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.