[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Control Plane Policer Information

#### Purpose

Display information about control plane policer for a specified protocol or all protocols.

#### Action

To display information about control plane policer:

    host1#show control-plane policer protocol
    Burst
                                          Rate   Size   Packets    Packets
              Protocol            Enabled (pps) (pkts) Committed   Exceeded
    ----------------------------- ------- ----- ------ ---------- ----------
    PppEchoRequest                  false    50     50          0          0
    PppEchoReply                    false    50     50          0          0
    PppEchoReplyFast                false    50     50          0          0
    PppControl                      false    50     50          0          0
    AtmControl                      false    50     50          0          0
    AtmOam                          false    50     50          0          0
    AtmDynamicIf                    false    50     50          0          0
    AtmInverseArp                   false    50     50          0          0
    FrameRelayControl               false    50     50          0          0
    FrameRelayArp                   false    50     50          0          0
    PppoeControl                    false    50     50          0          0
    PppoePppConfig                  false    50     50          0          0
    EthernetArp                     false    50     50          0          0
    EthernetArpMiss                 false    50     50          0          0
    EthernetLacp                    false    50     50          0          0
    EthernetDynamicIf               false    50     50          0          0

#### Meaning

Table 34 lists the show control-plane policer command output fields.

Table 34: show control-plane policer Output Fields

Field Name | Field Description
--- | ---
Protocol | Name of the protocol
Enabled | True or False
Rate (pps) | Rate, in packets per second in the range 0–10000
Burst Size (pkts) | Burst size, in packets, in the range 0–10000
Packets Committed | Number of packets committed
Packets Exceeded | Number of packets exceeded

#### Related Topics

- show control-plane policer

[Contents] [Prev] [Next] [Index] [Report an Error]