[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls ldp targeted-hello receive list

#### Syntax

[ no ] mpls ldp targeted-hello receive list
{ access-list accessListName | ipAddress [ ipAddress ]* }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the list of peer addresses from which MPLS accepts targeted hello messages. When you configurea receive list, hello messages are accepted only from list members. If no list is configured, hello messages are accepted from all addresses. The no version removes the list of peer addresses.

| Note: This command is unnecessary if you configure the mpls ldp targeted-hello send list command.

#### Options

- accessListName—String of up to 32 alphanumeric characters that identifies an access list
- ipAddress—IP address of a peer
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]