[Contents] [Prev] [Next] [Index] [Report an Error]

# ip rip receive version

#### Syntax

ip rip receive version { 1 | 2 | 1 2 | 2 1 | off }

no ip rip receive version

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Restricts the RIP version that the router can receive on an interface. The no version sets the interface back to the default value, receiving both RIP version 1 and version 2.

#### Options

- 1—Specifies RIP version 1 only
- 2—Specifies RIP version 2 only
- 1 2—Specifies RIP version 1 and version 2
- 2 1—Specifies RIP version 2 and version 1
- off—Turns reception off

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]