[Contents] [Prev] [Next] [Report an Error]

# T3 ATM Module Combination (4 Ports) (128 MB)

This module combination is no longer supported because the line module has reached end-of-life. However, the I/O module is still supported.

> Line module label | OCx/STMx ATM or OCx/STMx /DS3-ATM
> I/O module label | 4xDS3 ATM I/O
> Number of I/O ports | 4
> Software release | First supported: 4.1.0 Final supported: 5.2.x
> Description | 130 W Unchannelized T3 for ATM
> Type | ASIC
> Capability | ATM/AAL5
> Software features | See ERX Module Guide, Appendix A, Module Protocol Support for information about the layer 2 and layer 3 protocols and applications that this module combination supports.
> Model compatibility | ERX-7xx models ERX-14xx models ERX-310 router
> SRP module compatibility | SRP-5G+ SRP-10G SRP-40G SRP-40G PLUS SRP-SE10G
> Module redundancy support | 1:N redundancy
> Cables and connectors | 75-ohm connector The line interface unit supports two line buildouts: 0–68.5 m (0–225 feet) 69–137 m (226–450 feet) Signal strength is software controlled. The transmitted signal complies with ANSI T1.102-1993 Digital Hierarchy - Electrical Interfaces (1999) for cable lengths up to 201 m (660 feet).
> LEDs | See ERX Module Guide, Appendix B, Module LEDs.
> Alarms, errors, and events | See Monitoring Interfaces in the Configuring T3 and E3 Interfaces chapter of the JUNOSe Physical Layer Configuration Guide for Release 8.0.x and earlier.

[Contents] [Prev] [Next] [Report an Error]