> - Downloads
> - Specifying the Number of Retransmission Attempts
> - Related Topics
> - l2tp retransmission

> # Specifying the Number of Retransmission Attempts

> You can specify the number of retransmission attempts the router uses for tunnels, in the range 2–30. By default, the router uses a retry count of 5.

> Use the established keyword to apply the retry count only to established tunnels. Use the not-established keyword to apply the retry count only to tunnels that are not established. If you do not include a keyword, the router applies the retry count to both established and nonestablished tunnels.

> - To configure the number of retransmission attempts:
>   `
>   host1(config)#l2tp retransmission 4 established
>   `

> #### Published: 2009-10-07

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.