[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Tunnel-Server Ports and Tunnel-Service Interfaces

This section describes the tasks associated with configuring a tunnel-server port and tunnel-service interface.

## Identifying the Physical Location of the Tunnel-Server Port

To display the physical location of the dedicated tunnel-server port on your module, issue the show tunnel-server config command.

    host1#show tunnel-server config

                              Server Ports
                              ------------
                                             Provisioned
      Port      Type     MaximumInterfaces   Interfaces    HwPresent
    --------   -------   -----------------   -----------   ---------
    Port 2/2   shared       8000                0             yes
    Port 8/0   dedicated    16000               8000          yes

## Provisioning the Maximum Number of Interfaces on a Tunnel-Server Port

To provision the maximum number of interfaces on a tunnel-server port:

1. From Global Configuration mode, specify the location of the dedicated tunnel-server port that you want to configure.

   On a dedicated tunnel-server port:

   `
   host1(config)#tunnel-server 8/0
   host1(config-tunnel-server)#
   `

   On a shared tunnel-server port:

   `
   host1(config)#tunnel-server 2/2
   host1(config-tunnel-server)#
   `

   This command accesses Tunnel Server Configuration mode.

2. Provision the maximum number of tunnel-service interfaces to be used on the dedicated tunnel-server port.
   `
   host1(config-tunnel-server)#max-interfaces all-available
   `

   | Note: When you issue the tunnel-server command, ensure that you specify the same interface specifier that was displayed for this tunnel-server port in the show tunnel-server config command in the output described in Identifying the Physical Location of the Tunnel-Server Port. If you specify an incorrect location for the tunnel-server port, the router displays an error message and rejects the command as invalid.

## Verifying the Tunnel-Server Interface Configuration

To verify that you properly provisioned the number of tunnel-server interfaces on the tunnel-server port:

1. From Tunnel Server Configuration Mode, return to Privileged Exec mode.
   `
   host1(config-tunnel-server)#exit
   host1(config)#exit
   host1#
   `
2. Issue the show tunnel-server config command.

       host1#show tunnel-server config

                                 Server Ports
                                 ------------
                                                Provisioned
         Port      Type     MaximumInterfaces   Interfaces    HwPresent
       --------   -------   -----------------   -----------   ---------
       Port 2/2   shared       8000                5000          yes
       Port 8/0   dedicated    16000               all-available yes

   For more information about using the show tunnel-server command, see Monitoring Tunnel-Service Interfaces.

## Unprovisioning Tunnel-Service Interfaces

To unprovision the tunnel-service interfaces on a tunnel-server port, use any of the following commands, all of which have the same effect:

- Issue the no max-interfaces command from Tunnel Server Configuration mode.
  `
  host1(config-tunnel-server)#no max-interfaces
  `
- Issue the max-interfaces 0 command from Tunnel Server Configuration mode.
  `
  host1(config-tunnel-server)#max-interfaces 0
  `
- Issue the no tunnel-server command from Global Configuration mode. This command unprovisions the tunnel-service interfaces on the specified tunnel-server port but does not delete the port itself.
  `
  host1(config)#no tunnel-server 2/2
  `

max-interfaces

- Use from Tunnel Server Configuration mode to provision the maximum number of tunnel-service interfaces to be used on a tunnel-server port.
- Specify an integer in the range 0–16000 to provision the maximum number of tunnel-service interfaces.
- Use the all-available keyword to provision the maximum number of tunnel-service interfaces to match the maximum value that the tunnel-server module supports.
- Examples
  `
  host1(config-tunnel-server)#max-interfaces 5000
  host1(config-tunnel-server)#max-interfaces all-available
  `
- Use the default version to restore the default configuration. On dedicated tunnel-server ports, the default configuration is the maximum number of tunnel-service interfaces that the tunnel-service module supports (all-available). On shared tunnel-server ports, the default configuration is zero tunnel-server interfaces.
- Use the no version to reduce the number of provisioned tunnel-service interfaces to zero. Issuing the no max-interfaces command has the same effect as issuing the max-interfaces 0 command.
- See max-interfaces.

tunnel-server

- Use from Global Configuration mode to specify the physical location of the tunnel-server port that you want to configure.
- The tunnel-server command accesses Tunnel Server Configuration mode, which enables you to provision the maximum number of tunnel-service interfaces to be used on the tunnel-server port.
- For ERX7xx models, ERX14xx models, and the ERX310 router , use the slot/port format.
- For the E120 and E320 Broadband Services Routers, use the slot/adapter/port format. On dedicated tunnel-server ports, use adapter 0 and port 0. On shared tunnel-server ports, use adapter 2 and port 0.
- Example
  `
  host1(config)#tunnel-server 12/2
  `
- Use the default version to restore the default configuration. On dedicated tunnel-server ports, the default configuration is the maximum number of tunnel-service interfaces that the tunnel-service module supports. On shared tunnel-server ports, the default configuration is zero tunnel-service interfaces.
- Use the no version to reduce the number of provisioned tunnel-service interfaces to zero.
- See tunnel-server.

[Contents] [Prev] [Next] [Index] [Report an Error]