[Contents] [Prev] [Next] [Index] [Report an Error]

# ip igmp ssm-map static

#### Syntax

[ no ] ip igmp ssm-map static accessListName sourceAddress

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies an access list and source address for use in SSM mapping. SSM mapping statically assigns sources to IGMPv1 and IGMPv2 groups. You must use SSM mapping for IGMPv1 and IGMPv2 hosts to interoperate with PIM SSM. SSM mapping allows the router to use a statically configured list to translate (*,G) memberships to (S,G) memberships. The no version removes the SSM map association.

#### Options

- accessListName—Name of the access control list
- sourceAddress—Address of the source

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]