> - Downloads
> - show subscribers

> # show subscribers

> #### Syntax

> To display detailed information:

> show subscribers [ ipv6 [ ipv6Prefix ] ]
> [ domain domainName | icr-partition icrPartitionLocationId | interface { atm | ethernet }
> interfaceSpecifier | port interfaceSpecifier |
> slot slotNumber | username userName |
> virtual-router vrName ] [ filter ]

> To display summary information:

> show subscribers summary [ domain | icr-partition | interface | port | slot | virtual-router ]
> [ filter ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.
> interface, atm, and ethernet keywords added in JUNOSe Release 7.3.0.
> slot keyword and slotNumber variable added in JUNOSe Release 7.3.0.
> icr-partition keyword and icrPartitionLocationId variable added in JUNOSe Release 10.3.0.

> #### Description

> Displays the active subscribers on your router.

> #### Options

> - ipv6—Displays IPv6 subscribers for the domain
> - ipv6Prefix—Prefix that defines the IPv6 network that you want to filter
> - userName—Username of active subscriber
> - domain—Displays active subscribers for the domain
> - domainName—Domain name matching usernames of active subscribers
> - icr-partition—Displays active subscribers for the ICR partition
> - icrPartitionLocationId—A unique identifier for each ICR partition on a chassis. Note that this ID different from the partition ID, which is configured using the ip vrrp vrid icr-partition partitionId command. The partition location ID that you specify here is a combination of the interface within the chassis on which the ICR partition is configured and the VRRP ID, which is system-defined and nonconfigurable.
> - interface—Displays active subscribers for the the specified interface, atm or ethernet, or in the summary version, displays active subscribers for all ATM and Ethernet interfaces
> - interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
> - port—Displays active subscribers for the port
> - slot—Displays active subscribers for the slot
> - slotNumber—Number of the chassis slot of the line module in the range 0–2 (ERX310 model), 0–6 (ERX7xx models), 0–13 (ERX14xx models), 0-5 (E120 router), and 0-16 (E320 router)
> - virtual-router—Displays active subscribers for the VR
> - vrName—Name of the VR to which interfaces of active subscribers are bound
> - filter—See Filtering show Commands
> - summary—Displays the active subscribers for each domain, interface, port, slot, or virtual router

> #### Mode

> Privileged Exec

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.