[Contents] [Prev] [Next] [Index] [Report an Error]

# ip-hint

#### Syntax

ip-hint { enable | disable }

no ip-hint

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

When enabled, the E Series router preallocates an IP address for the remote (B-RAS) user before calling authentication. The address is then passed as a hint in the authentication request to the RADIUS server. The no version disables the feature.

#### Options

- enable—Specifies the feature
- disable—Disables the feature; this is the default setting

#### Mode

Domain Map Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]