[Contents] [Prev] [Next] [Index] [Report an Error]

## Index

A B C D F H I L M N O P R S T U V W

A

> Access-Request messages
>   ICR Partition ID VSA 1
> Acct-Start messages
>   ICR Partition ID VSA 1
> Acct-Stop messages
>   ICR Partition ID VSA 1
> assembly numbers, displaying for hardware 1
> assembly revisions, displaying for hardware 1
> automatic switchover 1

B

> backup router 1
>   defined 1
>   election process and 1
>   VRRP 1
> bandwidth
>   optimizing 1
> baseline commands
>   baseline ip vrrp 1

C

> clear commands
>   clear redundancy history 1
> conventions
>   notice icons 1
>   text and syntax 1
> customer support 1
>   contacting JTAC 1

D

> destination address (DA), VRRP 1
> disable-switch-on-error command 1
> documentation set
>   comments on 1

F

> failover. See switchover

H

> hardware
>   monitoring information 1, 2
> high availability
>   activating 1
>   deactivating 1
>   IP interface priority 1, 2
>   monitoring 1
>   overview 1

I

> icr cluster 1
> ICR commands
>   interface 1
> icr interface 1
> ICR Options
>   icr-control-interface 1
>   priority command 1
>   timers-learn command 1
> ICR Partition
>   configuring 1, 2, 3, 4, 5
>   configuring, naming 1
>   radius 1
> ICR partition accounting
>   and dependence on Acct-Stop messages 1
>   configuring 1
>   disabling and enabling messages
>     sent to the RADIUS server 1
>   overview 1
>   processing in different scenarios
>     administrative switchover 1
>     complete chassis failure 1
>     line module or interface failure 1
>     transition of ICR partition states 1
> ICR Partition commands
>   naming 1
> ICR partition ID VSA
>   including in access and accounting messages 1
> ICR Partition ID VSA
>   transmitting to the virtual router
>     where ICR control interface is configured 1
>     where ICR partition is configured 1
> ICR Partition Options
>   advertise-mac 1, 2
>   control-subinterface 1, 2
>   group option 1, 2
>   use-default-mac 1, 2
> ICR Partitions
>   configuration example
>     backup ICR partition, S-VLAN based grouping 1
>     master ICR partition, S-VLAN based grouping 1
> ICR RADIUS commands
>   inclusion of icr-partition-id 1
>   radius icr-partition-accounting 1
> icr-partition 1
> in-service software upgrade. See unified ISSU
> Interchassis Redundancy
>   heterogenous icr clusters 1
>   icr clusters 1
>   icr partition 1
> Interim-Acct messages
>   ICR Partition ID VSA 1
> IP addresses
>   IP address owner, VRRP 1
>   primary, VRRP 1
>   VRRP 1, 2
> ip commands 1
>   ip initial-sequence-preference 1
>   ip vrrp 1
>   ip vrrp accept-data 1
>   ip vrrp advertise-interval 1
>   ip vrrp authentication-key 1
>   ip vrrp authentication-type 1
>   ip vrrp enable 1, 2
>   ip vrrp preempt 1
>   ip vrrp priority 1, 2
>   ip vrrp track 1
>   ip vrrp virtual-address 1, 2
>   See also vrrp commands
> ip pim commands
>   ip pm dr-priority 1
> ipv6 commands
>   ipv6 initial-sequence-preference 1
> ISSU. See unified ISSU

L

> LEDs
>   monitoring status 1
> line module redundancy
>   configuring 1, 2
>   E120 and E320 Broadband Services Routers 1
>     IOA behavior 1
>   ERX7xx models and ERX14xx models 1
>   managing 1
>   monitoring 1

M

> manuals
>   comments on 1
> master router 1
> memory (hardware), displaying 1

N

> notice icons 1

O

> optimizing bandwidth 1
> overload advertise-high-metric issu command 1, 2

P

> physical slots
>   rebooting 1
> platform considerations
>   high availability 1

R

> RADIUS 1
> redundancy
>   line module. See line module redundancy
>   SRP module. See SRP module redundancy
> redundancy commands
>   redundancy force-switchover 1, 2
>   redundancy lockout 1
>   redundancy revert 1
>   redundancy revertive 1
> reversion
>   after switchover 1
> revisions, displaying assembly 1

S

> serial numbers, displaying for hardware 1
> Service Availability
>   Features 1
>   ICR 1
>   Module redundancy 1
>   Stateful SRP Switchover 1
>   Unified ISSU 1
>   VRRP 1
> show environment command 1
> show hardware command 1
> show icr commands
>   show icr-partition 1
>   show icr-partitions 1
>   state 1
>   summary 1
> show ip commands
>   show ip vrrp 1
>   show ip vrrp brief 1
>   show ip vrrp neighbors 1
>   show ip vrrp statistics 1
>   show ip vrrp statistics global 1
> show ip commands:show
>   ip interface 1
> show issu command 1
> show redundancy commands
>   show redundancy 1, 2, 3, 4
>   show redundancy clients 1
>   show redundancy switchover-history 1
> show version command 1
> software
>   upgrading 1
> SRP module redundancy 1
>   managing 1
>   monitoring 1
> SRP modules
>   installing a redundant module 1
>   reset button 1
> srp switch command 1
> stateful SRP switchover. 1
>   See also high availability
> status LEDs, monitoring 1
> support, technical See technical support
> switchover 1
> synchronize command 1, 2

T

> technical support
>   contacting JTAC 1
> text and syntax conventions 1

U

> unified ISSU (in-service software upgrade) 1
>   AAA support 1
>   application support 1
>   application-specific behavior 1
>   ATM support 1
>     ATM port date rate 1
>     ILMI sessions 1
>     OAM CC effects 1
>     OAM VC integrity 1
>     VC and VP statistics 1
>   DHCP support 1
>     common component 1
>     external server 1
>     packet capture 1
>     relay and relay proxy 1
>   DHCP support:relay and relay proxy 1
>   DoS protection support 1
>   Ethernet support 1
>     ARP entries 1
>     LAG 1
>     port data rate 1
>     VLAN statistics 1
>   FTP support 1
>   halting during initialization 1
>   halting during upgrade 1
>   initialization phase 1
>     application data on standby SRP module 1
>     line module arming 1
>     SNMP traps 1
>   IS-IS support 1
>     graceful restart 1
>     high link cost 1
>   L2TP support 1
>   layer 3 protocol traffic forwarding 1
>   monitoring 1
>   OSPF support 1
>     dead interval 1
>     graceful restart 1
>     high link cost 1
>   overview 1
>   phases
>     initialization 1
>     overview of 1
>     service restoration 1
>     upgrade 1
>   PIM support 1
>   platform 1
>   procedure for upgrade 1, 2
>   references 1
>   requirements
>     hardware 1, 2
>     software 1
>     traffic forwarding 1
>     verification in upgrade phase 1
>   restoring original router state 1
>   router behavior 1
>   service restoration phase 1
>   SONET/SDH support 1
>   subscriber support 1
>     logins 1
>     statistics 1
>   support, application 1
>   T3 support 1
>   TACACS+ support 1
>   terms 1
>   timer settings for routing protocol timers 1
>   upgrade phase 1
>     exceptions 1
>     line module control plane 1
>     line module forwarding plane upgrade 1
>     process steps 1
>     setup 1
>     SRP module switchover 1
>     verification requirements 1
>   upgrade procedure 1
> unified ISSU (in-service software upgrade):DHCP support
>   local server 1
> upgrading software 1

V

> virtual MAC address 1
> virtual router ID (VRID). See VRID
> Virtual Router Redundancy Protocol (VRRP). See VRRP
> VRID (virtual router ID)
>   configuration 1
>   creating 1, 2
>   router election rules 1
> VRRP 1
> VRRP (Virtual Router Redundancy Protocol)
>   advertisement interval 1
>   advertisement messages 1
>   authentication key 1
>   authentication type 1
>   backup router 1, 2, 3
>   configuration examples 1
>   configuring 1
>   how it works 1
>   implementation 1, 2
>   MAC address 1
>   master router 1
>   monitoring 1
>   overview 1
>   preemption 1, 2
>   router election rules 1
>   router priority 1
>   VLAN support 1
>   VRRP router defined 1
> vrrp commands
>   ip vrrp 1
>   ip vrrp accept-data 1
>   ip vrrp advertise-interval 1
>   ip vrrp authentication-key 1
>   ip vrrp authentication-type 1
>   ip vrrp enable 1, 2
>   ip vrrp preempt 1, 2
>   ip vrrp priority 1
>   ip vrrp track 1
>   ip vrrp virtual-address 1
> VRRP commands
>   icr 1

W

> warm restart
>   IP interface priority during 1, 2

[Contents] [Prev] [Next] [Index] [Report an Error]