[Contents] [Prev] [Next] [Index] [Report an Error]

# Specifying the Number of Retransmission Attempts

You can specify the number of retransmission attempts the router uses for tunnels, in the range 2–30. By default, the router uses a retry count of 5.

Use the established keyword to apply the retry count only to established tunnels. Use the not-established keyword to apply the retry count only to tunnels that are not established. If you do not include a keyword, the router applies the retry count to both established and nonestablished tunnels.

- To configure the number of retransmission attempts:
  `
  host1(config)#l2tp retransmission 4 established
  `

#### Related Topics

- l2tp retransmission

[Contents] [Prev] [Next] [Index] [Report an Error]