> - Downloads
> - restricted
> - Related Topics
> - Configuring Interface Supersets for QoS

> # restricted

> #### Syntax

> [ no ] restricted interface restrictedInterfaceType interfaceSpecifier [ atmVpi | s-vlanIdValue ]

> #### Release Information

> Command introduced in JUNOSe Release 9.2.0.

> #### Description

> Configures an interface superset as restricted to a particular ATM-VPI or S-VLAN ID. The no version deletes the restriction for the interface superset.

> #### Options

> - restrictedInterfaceType—One of the following restricted interface types: atm-vp, fastEthernet, gigabitEthernet, svlan, tenGigabitEthernet
> - interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers in About This Guide
> - atmVpi—Virtual path identifier of this PVC; number in the range 0–255
> - s-vlanIdValue—S-VLAN ID number in the range 0–4095

> #### Mode

> QoS Interface Superset Configuration

> #### Published: 2009-10-08

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.