[Contents] [Prev] [Next] [Index] [Report an Error]

# ip vrrp icr-partition group

#### Syntax

ip vrrp vrid icr-partition group partitionGroupingType

#### Release Information

Command introduced in JUNOSe Release 10.3.0.

#### Description

Configures the ICR partition to use either S-VLAN-based grouping or VLAN-based grouping for subscribers. If you specify VLAN as the grouping type or partition type, the ICR partition consists of single-tagged VLAN-based subinterfaces. By default, the ICR partition uses S-VLAN-based grouping. There is no no version.

#### Options

- vrid—VRID identifier; a number in the range 1–255
- partitionGroupingType—One of the following partition types:
  - svlan—Configures the ICR partition to use double-tagged S-VLAN based subinterfaces.
  - vlan—Configures the ICR partition to use single-tagged VLAN based subinterfaces.

#### Mode

Interface Configuration, Subinterface Configuration

#### Related Topics

- Grouping ICR Subscribers Based on S-VLAN IDs
- Grouping ICR Subscribers Based on VLAN IDs
- Configuring an ICR Partition

[Contents] [Prev] [Next] [Index] [Report an Error]