> - Downloads
> - pppoe max-session-vsa

> # pppoe max-session-vsa

> #### Syntax

> pppoe max-session-vsa { override | ignore }

> no pppoe max-session-vsa override

> #### Release Information

> Command introduced in JUNOSe Release 9.3.0.

> #### Description

> Configures the PPPoE application to override the current PPPoE maximum session value set with the pppoe sessions command with the PPPoE maximum session value returned by the RADIUS server in the Max-Clients-Per-Interface VSA [26-143] in Access-Accept messages. The no version restores the default behavior, which ignores the PPPoE maximum session value returned by RADIUS.

> | Note: The router never overrides the maximum number of PPPoE subinterfaces supported per line module with a value from RADIUS that is either 0 (zero) or greater than the maximum number of supported PPPoE subinterfaces. See JUNOSe Release Notes, Appendix A, System Maximums corresponding to your software release for information about the maximum number of PPPoE subinterfaces supported for each line module.

> #### Mode

> Interface Configuration, Profile Configuration, Subinterface Configuration

> #### Published: 2009-10-08

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.