[Contents] [Prev] [Next] [Index] [Report an Error]

# reload slot

#### Syntax

reload slot slotNumber [ subsystem ] [ force ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Reboot the module in the selected slot. You can reboot the subsystems on the SRP modules on the E120 router or the E320 router separately. There is no no version.

#### Options

- slotNumber—Number of a selected slot in the router; for ERX7xx models, a number, in the range 0–6; for ERX14xx models, a number, in the range 0–13; for the ERX310 router, a number, in the range 0–2; for E120 and E320 routers, a number, in the range 0–16
- subsystem—Type of subsystem on E120 and E320 routers; use when the specified slotNumber is a slot that contains an SRP module
  - srp—Indicates the system controller (SC) on one or both SRP modules; specify this keyword to reboot only the portion of the SC on the individual SRP module
  - fabric—Indicates the portion of the switch fabric on the SRP modules; specify this keyword to reboot only an individual fabric slice
- force—Prompts for confirmation to reboot if the router is in certain states, such as during the synchronization of SRP modules, that could lead to a loss of configuration data or an NVS corruption.

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]