> - Downloads
> - instance-interface-type
> - Related Topics
> - Configuring a Basic Parameter Definition for QoS Administrators
> - Creating a QoS Parameter on an Interface Superset or Interface Set

> # instance-interface-type

> #### Syntax

> instance-interface-type {instanceInterfaceType | set | superset }

> no instance-interface-type { instanceInterfaceType | all }

> #### Release Information

> Command introduced in JUNOSe Release 7.1.0.
> lag keyword added in JUNOSe Release 8.1.0.

> set and superset keywords added in JUNOSe Release 9.2.0.

> #### Description

> Assigns an instance-interface type to a QoS parameter definition. Instance-interface types indicate the interfaces for which QoS clients can assign QoS parameter instances. You can specify up to eight instance-interface types for each parameter definition. The no version removes the specified instance-interface type from the parameter definition.

> #### Options

> - instanceInterfaceType—One of the following instance-interface types: atm, atm-vc, atm-vp, bridge, ethernet, fr-vc, ip, ip-tunnel, ipv6, lag, l2tp-session, l2tp-tunnel, lsp, pppoe, serial, server-port, svlan, vlan
> - set—Specifies an interface set as an instance-interface type
> - superset—Specifies an interface superset as an instance-interface type
> - all—Removes all instance-interface types

> #### Mode

> QoS Parameter Definition

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.