> - Downloads
> - node
> - Related Topics
> - Configuring a QoS Profile
> - Configuring Shadow Nodes
> - Configuring a Basic Parameter Definition for QoS Administrators
> - Attaching a QoS Profile to an Interface Superset or an Interface Set

> # node

> #### Syntax

> [ no ] { typeOfInterface | set | superset } node [ group trafficClassGroup | scheduler-profile
> schedulerProfileName ]*

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.
> svlan keyword added in JUNOSe Release 7.1.0.

> set and superset keywords added in JUNOSe Release 9.2.0.

> #### Description

> Specifies that a scheduler node be configured for each interface of the given interface type. The no version removes this rule from the QoS profile.

> #### Options

> - typeOfInterface—Interface types for scheduler nodes to be configured: atm, atm-vc, atm-vp, bridge, ethernet, fr-vc, ip, ip-tunnel, ipv6, l2tp-session, l2tp-tunnel, lsp, serial, server-port, svlan, vlan
> - set—Configures the node for an interface set
> - superset—Configures the node for an interface superset
> - trafficClassGroup—Name of the traffic class group
> - schedulerProfileName—Name of the scheduler profile
> - *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

> #### Mode

> QoS Profile Configuration

> #### Published: 2009-10-08

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.