[Contents] [Prev] [Next] [Index] [Report an Error]

# sscc option

#### Syntax

sscc option user-ip-mask-override

no sscc option

#### Release Information

Command introduced in JUNOSe Release 10.2.0.

#### Description

Enables user IP address mask to be sent to Policy Decision Point (PDP) in place of the interface IP address mask for a virtual router. If user IP address mask is not available, then the interface IP address mask is sent. The no version disables user IP address mask override.

#### Options

- user-ip-mask-override—Enables user IP address mask to be sent to PDP.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]