[Contents] [Prev] [Next] [Index] [Report an Error]

# rd

#### Syntax

rd distinguisher

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the unique two-part route distinguisher for a VRF. There is no no version.

#### Options

- distinguisher—Unique two-part identifier in the format number1:number2
  - number1—AS number or an IP address
  - number2—Unique integer; 32 bits if number1 is an AS number; 16 bits if number1 is an IP address

#### Mode

VRF Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]