> - Downloads
> - show qos-parameter
> - Related Topics
> - Monitoring QoS Parameter Instances

> # show qos-parameter

> #### Syntax

> To display settings for a specific parameter instance with references:

> show qos-parameter [ qosParameterInstanceName ] references [ brief | full ] [ filter ]

> To display references globally:

> show qos-parameter [ qosParameterInstanceName ] references global
> [ qosParameterInstanceName ] [ brief | full ] [ filter ]

> To display references for interfaces:

> `
> show qos-parameter [ qosParameterInstanceName ] references [ interface interfaceType interfaceSpecifier [ atmVpi | s-vlanIdValue ] ] [ explicit ] [ brief | full ]
> [ filter ]
> `

> To display references for L2TP sessions:

> show qos-parameter [ qosParameterInstanceName ] references lt2p session sessionName [ explicit ] [ filter ]

> #### Release Information

> Command introduced in JUNOSe Release 7.1.0.
> full keyword added in JUNOSe Release 7.2.0.

> #### Description

> Displays QoS parameter instance settings for QoS clients.

> #### Options

> - qosParameterInstanceName—Name of the parameter instance
> - references—Displays interfaces that reference this parameter instance
> - global—Displays information about global parameter instances
> - interfaceType—Interface type; see Interface Types and Specifiers
> - interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
> - atmVpi—Virtual path identifier of this PVC; number in the range 0–255
> - s-vlanIdValue—S-VLAN ID number in the range 0–4095
> - sessionName —Name of the L2TP session
> - brief—Displays information in a condensed format
> - full—Displays information in expanded format
> - explicit—Displays parameter instances only on the specified interface and not parameter instances stacked above the interface
> - filter—See Filtering show Commands

> #### Mode

> Privileged Exec, User Exec

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.