> - Downloads
> - sscc option

> # sscc option

> #### Syntax

> sscc option user-ip-mask-override

> no sscc option

> #### Release Information

> Command introduced in JUNOSe Release 10.2.0.

> #### Description

> Enables user IP address mask to be sent to Policy Decision Point (PDP) in place of the interface IP address mask for a virtual router. If user IP address mask is not available, then the interface IP address mask is sent. The no version disables user IP address mask override.

> #### Options

> - user-ip-mask-override—Enables user IP address mask to be sent to PDP.

> #### Mode

> Global Configuration

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.