> - Downloads
> - ip vrrp icr-partition group
> - Related Topics
> - Grouping ICR Subscribers Based on S-VLAN IDs
> - Grouping ICR Subscribers Based on VLAN IDs
> - Configuring an ICR Partition

> # ip vrrp icr-partition group

> #### Syntax

> ip vrrp vrid icr-partition group partitionGroupingType

> #### Release Information

> Command introduced in JUNOSe Release 10.3.0.

> #### Description

> Configures the ICR partition to use either S-VLAN-based grouping or VLAN-based grouping for subscribers. If you specify VLAN as the grouping type or partition type, the ICR partition consists of single-tagged VLAN-based subinterfaces. By default, the ICR partition uses S-VLAN-based grouping. There is no no version.

> #### Options

> - vrid—VRID identifier; a number in the range 1–255
> - partitionGroupingType—One of the following partition types:
>   - svlan—Configures the ICR partition to use double-tagged S-VLAN based subinterfaces.
>   - vlan—Configures the ICR partition to use single-tagged VLAN based subinterfaces.

> #### Mode

> Interface Configuration, Subinterface Configuration

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.