[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring QoS Parameters for Service Manager

#### Purpose

Display the Service Manager references for parameters for QoS clients.

#### Action

To display information in expanded format, including Service Manager references:

    host1#show qos-parameter video references full
                                               service
                       parameter               manager
        interface        name    value source   refs   persistence
    ------------------ --------- ----- ------- ------- -----------
    GigabitEthernet6/0 video      50   default  none    persistent

      Global parameter instances:   0
      Parameter instances reported: 1

#### Meaning

Table 158 lists the show qos-parameter command output fields.

Table 158: show qos-parameter Output Fields

Field Name | Field Description
--- | ---
interface | Location of the interface to which the parameter instance is assigned; global indicates that the parameter is assigned to the chassis
parameter name | Name of the parameter instance
value | Value assigned to the parameter instance
source | Source of the parameter instance: dcm—Parameter instance was created in a profile radius—Parameter instance was created through RADIUS service manager—Parameter instance was created through Service Manager default—Parameter instance was created through the CLI or SNMP
service manager refs | Number of references of this parameter instance created through Service Manager
persistence | Status of the persistence of a parameter instance in the system:persistent—Parameter instance is stored in NVS and is restored after a chassis reset non-persistent—Parameter instance is not stored in NVS and are deleted after a chassis reset
Global parameter instances | Number of parameter instances assigned to the chassis
Parameter instances reported | Total number of parameter instances assigned
Explicit parameter instances | Total number of explicit parameter instances assigned
Hierarchical parameter instances | Total number of hierarchical parameter instances assigned
IP multicast parameter instances | Total number of parameter instances associated with the IP multicast bandwidth adjustment application

#### Related Topics

- show qos-parameter

[Contents] [Prev] [Next] [Index] [Report an Error]