[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 nd ns-interval

#### Syntax

ipv6 nd ns-interval milliseconds

no ipv6 nd ns-interval

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the interval between IPv6 neighbor solicitation retransmissions on an interface. The no version returns the interval between neighbor solicitation retransmission to its default value (zero [0] milliseconds for router advertisements and 1000 milliseconds for Neighbor Discovery activity of the E Series router).

#### Options

- milliseconds—Interval between IPv6 neighbor solicit transmissions

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]