[Contents] [Prev] [Next] [Index] [Report an Error]

# ip vrrp advertise-interval

#### Syntax

ip vrrp vrid advertise-interval advertiseInterval [ seconds | milliseconds ]

no ip vrrp vrid advertise-interval

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the VRRP advertisement interval time. You must use seconds to comply with RFC 2338. Use milliseconds only if all VRRP instances peering for the given VRID are composed of E Series routers. The no version restores the default value, 1 second.

#### Options

- vrid—VRID identifier; a number in the range 1–255
- advertiseInterval—Advertisement period in seconds or milliseconds; in the range 1–255 seconds or 100–255000 milliseconds
- seconds—Specifies interval in seconds
- milliseconds—Specifies interval in milliseconds

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]