> - Downloads
> - timeout

> # timeout

> #### Syntax

> RADIUS:

> timeout waitTime

> no timeout

> RTR:

> timeout timeoutValue

> no timeout

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> When used from RADIUS Configuration mode, specifies the interval, in seconds, before the router retransmits a RADIUS packet to an authentication or accounting server. The no version restores the default.

> When used from RTR Configuration mode, specifies the timeout for a Response Time Reporter operation. The no version returns the operation to the default value. You can apply this parameter only to echo entries.

> #### Options

> - waitTime—Number of seconds in the range 1–1000; default value is 3
> - timeoutValue—Number in milliseconds that the operation waits for a response; if the value is set to 0 or is larger than frequency, it will be ignored; default value is 5000

> #### Mode

> RADIUS Configuration, RTR Configuration

> #### Published: 2009-10-09

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.