> - Downloads
> - radius dsl-port-type

> # radius dsl-port-type

> #### Syntax

> radius dsl-port-type { sdsl | adsl-cap | adsl-dmt | idsl | xdsl | virtual }

> no radius dsl-port-type

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Sets RADIUS attribute 61, NAS-Port-Type, in RADIUS access request packets and accounting start and stop packets for ATM interfaces. The no version restores the default setting, xdsl.

> #### Options

> - sdsl—Symmetric DSL
> - adsl-cap—Asymmetric DSL, carrierless amplitude phase modulation
> - adsl-dmt—Asymmetric DSL, discrete multitone
> - idsl—ISDN DSL
> - xdsl—DSL of unspecified type (default)
> - virtual—Virtual

> #### Mode

> Global Configuration

> #### Published: 2009-10-08

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.