> - Downloads
> - profile

> # profile

> #### Syntax

> To assign a profile name for a remote host:

> [ no ] profile profileName

> To create a profile or assign a profile to an interface:

> profile [ bridgedEthernet | ip | l2tp | ppp | pppoe | vlan | any ] profileName

> no profile [ bridgedEthernet | ip | l2tp | ppp | pppoe | vlan | any ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.
> vlan keyword added in JUNOSe Release 7.1.0.
> IP Tunnel Destination Profile Configuration mode added in JUNOSe Release 8.2.0.

> #### Description

> When used from Global Configuration mode, creates a profile. Use profiles to configure interfaces dynamically, which enables you to manage a large number of interfaces effectively. The no version removes the profile.

> When used from Interface Configuration mode and Subinterface Configuration mode, assigns a profile to an interface. Use profiles to configure interfaces dynamically, which enables you to manage a large number of interfaces effectively. The no version removes the profile assigned to the interface.

> When used in IP Tunnel Destination Profile Configuration mode, defines an IP profile with parameters that are used to stack an upper IP interface over a dynamic GRE or DVMRP tunnel. The no version removes the IP profile from the destination profile.

> When used from L2TP Destination Profile Host Configuration mode, sets an attribute of the current remote host. The no version removes the attribute from the remote host.

> #### Options

> - bridgedEthernet—Specifies a bridged Ethernet encapsulation type to which the profile applies
> - ip—Specifies an IP encapsulation type to which the profile applies
> - l2tp—Specifies an L2TP encapsulation type to which the profile applies
> - ppp—Specifies a PPP encapsulation type to which the profile applies
> - pppoe—Specifies a PPPoE encapsulation type to which the profile applies
> - vlan—Specifies a VLAN encapsulation type to which the profile applies
> - any—Specifies any autoconfigured encapsulation that does not have a specific profile assignment
> - profileName—Profile name of up to 80 characters

> #### Mode

> Global Configuration, Interface Configuration, IP Tunnel Destination Profile Configuration, L2TP Destination Profile Host Configuration, Subinterface Configuration

> #### Published: 2009-10-08

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.