> - Downloads
> - Monitoring the Configuration of QoS Interface Supersets
> - Related Topics
> - Configuring Interface Supersets for QoS
> - show qos-interface-superset

> # Monitoring the Configuration of QoS Interface Supersets

> #### Purpose

> Display information about configured interface supersets.

> #### Action

> To display information about a specific interface superset:

>     host1#show qos-interface-superset vlan-ss
>     interface           member restricted
>     superset    port    count  interface
>     --------- --------- ------ ----------
>     vlan-ss   lag test1   1     none

> To display detailed information about a specific interface superset:

>     host1#show qos-interface-superset vlan-ss detail
>     interface           member restricted
>     superset    port    count  interface
>     --------- --------- ------ ----------
>     vlan-ss    lag test1   1      none

>     Children:
>       set set

> #### Meaning

> Table 1 lists the show qos-interface-superset command output fields.

> Table 1: show qos-interface-superset Output Fields

> Field Name | Field Description
> --- | ---
> interface superset | Name of the interface superset
> port | Interface that is the parent of the interface superset
> member count | Number of interface members associated with the interface superset
> restricted interface | Restricted interface configured for this interface superset
> Children | List of interface set members associated with the interface superset

> #### Published: 2009-09-24

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.