> - Downloads
> - Monitoring the Configuration of the HTTP Local Server
> - Related Topics
> - show ip http server

> # Monitoring the Configuration of the HTTP Local Server

> #### Purpose

> Display information about the configuration of the HTTP local server.

> #### Action

> To display information about the HTTP local server:

>     host1#show ip http server
>       Admin status: enabled
>       Access class: not defined
>       Listening port: 80
>       Same host limit: 3
>       Protocol: IPv6

> #### Meaning

> Table 1 lists the show ip http server command output fields.

> Table 1: show ip http server Output Fields

> Field Name | Field Description
> --- | ---
> Admin status | Status of the HTTP local server in the software: enabled or disabled. Enabled implies that the HTTP local server can listen for IPv4 , IPv6, or both IPv4 and IPv6 exception packets.
> Access class | Name of a standard IP access list that determines which hosts can log on to the HTTP local server
> Listening port | Port that the HTTP local server uses to track requests for connection
> Same host limit | Maximum number of connections allowed between one IP address and the HTTP local server
> Protocol | Protocols that the HTTP local server is listening for: IPv4, IPv6, or IPv4 and IPv6.

> #### Published: 2009-10-07

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.