[Contents] [Prev] [Next] [Index] [Report an Error]

# set qos-bandwidth

#### Syntax

set qos-bandwidth { bandwidthValue | adaptive }

no set qos-bandwidth

#### Release Information

Command introduced in JUNOSe Release 7.1.0.
adaptive keyword added in JUNOSe Release 7.2.0.

#### Description

Sets a multicast bandwidth for QoS adjustment or defines the bandwidth as adaptive (automatically sensed). The no version removes the set clause from a route map.

#### Options

- bandwidthValue—Number, in the range 0–4294967259 kilobits per second, used for QoS adjustment
- adaptive—Defines the QoS bandwidth as being automatically sensed

#### Mode

Route Map Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]