[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Packet Mirroring Subscriber Information

#### Purpose

Display CLI-based packet mirroring information about the subscribers for whom packet mirroring is currently active. This command and the output are visible only to authorized users—the mirror-enable command must be enabled before using this command.

#### Action

To display information about subscribers for whom packet mirroring is active:

    host1# show mirror subscribers
    Subscriber ID                  Subscriber ID       Secure Policy  Secure Policy List  Sessions
                                   Method              Type                               Mirrored
    ------------------             ------------------  -------------  ------------------  --------
    vpn: fred@isp100.com           username            l2tp           securePolicyL2tp    1
    5551212                        calling station id  ip             securePolicyVpn     1
    erx atm 2/1/0.1:0.101:00010485 acct-session-id   	IPV6     		spl_8800000F   		1

#### Meaning

Table 64 lists show mirror subscribers command output fields.

Table 64: show mirror subscribers Output Fields

Field Name | Field Description
--- | ---
Subscriber ID | Subscriber being mirrored
Subscriber ID Method | Method used to identify the subscriber
Secure Policy Type | Type of secure policy; IP, IPv6, or L2TP
Secure Policy List | Name of secure policy list used for packet mirroring
Sessions Mirrored | Number of sessions being mirrored

#### Related Topics

- show mirror subscribers

[Contents] [Prev] [Next] [Index] [Report an Error]